|  |
| --- |
|  |
| **2018 Editorial Changes** |

The following items were deemed editorial in nature based on the following criteria: 1) the modified text did not change the meaning or procedure outlined, 2) modified text corrected an omission or clarified how the text was written, or 3) the item itself was reformatted and relocated in the text to make the organization of the content more meaningful.

**Note:**  For the purposes of this table, the **bold, underscored** text indicates new language added and **bold, ~~strikeout~~** text indicates deleted text.

| **Chapter** | **Section** | **Action** | **Page** |
| --- | --- | --- | --- |
|  | 3.9.2.2. Test Procedure | Clarified the instruction to read 2. Open each package **~~in turn, remove~~** and pour the contents **from a height of 2 ft~~, and pass them~~** through the . . . | 69 |
| 3.11.2. Test Procedure | Corrected the instruction in 11. *Product Density = (****~~gross weight in Step 5~~product net weight in Step 10)*** *÷ (the total water volume in Step 7* ***– volume of tare material in Step 8****)* | 74 |
| 3.13.2. Test Procedure  b. Test Procedure for Cylinders Labeled by Volume | 5. Updated the reference to NIST Standard Reference Data Base 23 “Reference Fluid Thermodynamic and Transport Properties Database” (REFPROP) | 81 |
| **3.14.3. Field Audit Procedure – Bundled and Bagged Firewood** | 3.14.3. Evaluation Results was broken into two sections. “Field Audit Procedure” is now “3.14.3. | 94 |
| **~~3.14.3.~~** **3.14.4.** **~~Evaluation of Results~~** became **Test Procedures** | This item was renumbered. | 96 |
| 3.15.1. Test Equipment | Corrected referenced table number. | 100 |
| 3.15.2. Test Procedure | Corrected note in “5. Volume Determination.” | 105 |
| Chapter 3. Test Procedures – For Packages Labeled by Volume | 3.15.2. Test Procedure. | 3.15.2. Test Procedure was broken into two sections. Line 7 was renumbered to “3.15.3. Evaluation of the Test Results and Determination of Pass or Fail” and the following information renumbered and formatted. | 105 |
| **3.15.3. Evaluation of the Test Results and Determination of Pass or Fail** | This section was split from 3.15.2. Test Procedure. | 115 |
| Chapter 4. Test Procedures – Packages Labeled by Count, Linear Measure, Area, Thickness, and Combinations of Quantities | 4.3.1. Test Equipment | Corrected omission of “**1/16**” in divisions… | 122 |
| 4.4. Special Test Requirements for Packages Labeled by Linear or Square Measure (Area) | Updated ASTM Reference | 124 |
| 4.5.2. Test Procedures  (a) Test Procedure for Polyethylene Sheeting | Made an editorial change to harmonize the content with the NIST Handbook 130 changes. | 125 |
| Appendix A. Tables | Table 2-10. Exceptions to the Maximum Allowable Variations for Textiles, Polyethylene Sheeting and Film, Mulch and Soil Labeled by Volume, Packaged Firewood **and Stove Wood Labeled by Volume**, and Packages Labeled by Count with 50 Items or Fewer, and Specific Agricultural Seeds Labeled by Count. | Title Correction omitted during the 2016 updates. | 157 |
| Appendix E. General Tables of Units of Measurement | Avoirdupois Units of Mass | Added parentheses around “or long”:  20 gross (or long) hundredweights = 1 gross (or long) ton | 201 |