# Table of Contents

**Page**

[Section 4.46. Berry Baskets and Boxes 4-39](#_Toc273451826)

[A. Application 4-39](#_Toc273451827)

[A.1. General. 4-39](#_Toc273451828)

[A.2. Additional Code Requirements. 4-39](#_Toc273451829)

[S. Specifications 4-39](#_Toc273451830)

[S.1. Units. 4-39](#_Toc273451831)

[S.2. Materials. 4-39](#_Toc273451832)

[S.3. Capacity Point. 4-39](#_Toc273451833)

[N. Notes 4-39](#_Toc273451834)

[N.1. Method of Test. 4-39](#_Toc273451835)

[T. Tolerances 4-39](#_Toc273451836)

[T.1. Tolerances on Individual Measures. 4-39](#_Toc273451837)

[T.2. Tolerances on Average Capacity. 4-39](#_Toc273451838)

THIS PAGE INTENTIONALLY LEFT BLANK

# Section 4.46. Berry Baskets and Boxes

## A. Application

### A.1. General.

 – This code applies to baskets and boxes for berries and small fruits in capacities of 1 dry quart and less.

### A.2. Additional Code Requirements.

 – In addition to the requirements of this code, berry baskets and boxes shall meet the requirements of Section 1.10. General Code.

## S. Specifications

### S.1. Units.

 – The capacity of a berry basket or box shall be ½ dry pint, 1 dry pint, or 1 dry quart.

### S.2. Materials.

 – A berry basket or box shall be made of any suitable materials that will retain its shape during normal filling, storage, and handling.

### S.3. Capacity Point.

 – The capacity of a berry basket or box shall be determined by its top edges.

## N. Notes

### N.1. Method of Test.

 – A berry basket or box may be tested either volumetrically, using rape seed as the testing medium, or geometrically through accurate inside dimension measurement and calculation.

## T. Tolerances

### T.1. Tolerances on Individual Measures.

 – Maintenance and acceptance tolerances in excess and deficiency on an individual measure shall be as shown in Table 1. Maintenance and Acceptance Tolerances in Excess and in Deficiency.

### T.2. Tolerances on Average Capacity.

 – The average capacity on a random sample of 10 measures selected from a lot of 25 or more shall be equal to or greater than the nominal capacity.

(Amended 1979)

|  |
| --- |
| **Table 1.****Maintenance and Acceptance Tolerances in Excess and in Deficiency** |
| **Nominal Capacity** | **Tolerance** |
| **In Excess****Cubic Inches** | **In Deficiency****Cubic Inches** |
| ½ pint | 1 | 0.5 |
| 1 pint | 2 | 1.0 |
| 1 quart | 3 | 1.5 |

THIS PAGE INTENTIONALLY LEFT BLANK