surface_treatment_thermal

EXPRESS specification:

ENTITY surface_treatment_thermal
SUBTYPE OF ( | surface_treatment);
initial_temperature | : | thermodynamic_temperature_measure_with_unit;
final_temperature | : | thermodynamic_temperature_measure_with_unit;
maximum_temperature | : | thermodynamic_temperature_measure_with_unit;
END_ENTITY;

References (2):

Name | Type | Referred through | Express-G
surface_treatment | Entity |
Subtype
| No Diagram
surface_treatment_thermal_timed | Entity |
Supertype
| No Diagram

Inheritance graph

ENTITY surface_treatment_thermal;
ENTITY structural_frame_item;
item_number | : | INTEGER;
item_name | : | label;
item_description | : | OPTIONAL text;
DERIVE
item_ref | : | BAG OF identifier := get_item_ref(SELF);
cost_code | : | BAG OF label := get_item_cost_code(SELF);
object_id | : | globally_unique_id := get_instance_id(SELF);
ENTITY structural_frame_process;
place_of_process | : | OPTIONAL organizational_address;
ENTITY surface_treatment;
surface_finish_specification | : | text;
ENTITY surface_treatment_thermal;
initial_temperature | : | thermodynamic_temperature_measure_with_unit;
final_temperature | : | thermodynamic_temperature_measure_with_unit;
maximum_temperature | : | thermodynamic_temperature_measure_with_unit;
END_ENTITY;