section_properties_asymmetric

EXPRESS specification:

ENTITY section_properties_asymmetric
SUBTYPE OF ( | section_properties);
neutral_axis_shear_centre | : | ARRAY [1:2] OF length_measure_with_unit;
theta_angle_z_axis_v_axis | : | OPTIONAL plane_angle_measure_with_unit;
inertia_moment_iu | : | OPTIONAL inertia_measure_with_unit;
inertia_moment_iv | : | OPTIONAL inertia_measure_with_unit;
radius_of_gyration_ru | : | OPTIONAL positive_length_measure_with_unit;
radius_of_gyration_rv | : | OPTIONAL positive_length_measure_with_unit;
section_modulii | : | ARRAY [1:8] OF modulus_measure_with_unit;
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
section_properties | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY section_properties_asymmetric;
ENTITY section_properties;
profile | : | section_profile;
origin_offset | : | ARRAY [1:2] OF length_measure_with_unit;
torsional_constant_ix | : | OPTIONAL inertia_measure_with_unit;
inertia_moment_iy | : | OPTIONAL inertia_measure_with_unit;
inertia_moment_iz | : | OPTIONAL inertia_measure_with_unit;
section_area_ax | : | OPTIONAL area_measure_with_unit;
shear_area_asy | : | OPTIONAL area_measure_with_unit;
shear_area_asz | : | OPTIONAL area_measure_with_unit;
shear_deformation_area_ay | : | OPTIONAL area_measure_with_unit;
shear_deformation_area_az | : | OPTIONAL area_measure_with_unit;
surface_per_length | : | OPTIONAL positive_length_measure_with_unit;
radius_of_gyration_ry | : | OPTIONAL positive_length_measure_with_unit;
radius_of_gyration_rz | : | OPTIONAL positive_length_measure_with_unit;
plastic_modulus_sy | : | OPTIONAL modulus_measure_with_unit;
plastic_modulus_sz | : | OPTIONAL modulus_measure_with_unit;
warping_constant | : | OPTIONAL derived_measure_with_unit;
torsional_index | : | OPTIONAL REAL;
buckling_parameter | : | OPTIONAL REAL;
nominal_mass | : | OPTIONAL mass_per_length_measure_with_unit;
actual_mass | : | OPTIONAL mass_per_length_measure_with_unit;
DERIVE
y_offset | : | REAL := NVL(origin_offset[1].value_component, 0.0);
z_offset | : | REAL := NVL(origin_offset[2].value_component, 0.0);
ENTITY section_properties_asymmetric;
neutral_axis_shear_centre | : | ARRAY [1:2] OF length_measure_with_unit;
theta_angle_z_axis_v_axis | : | OPTIONAL plane_angle_measure_with_unit;
inertia_moment_iu | : | OPTIONAL inertia_measure_with_unit;
inertia_moment_iv | : | OPTIONAL inertia_measure_with_unit;
radius_of_gyration_ru | : | OPTIONAL positive_length_measure_with_unit;
radius_of_gyration_rv | : | OPTIONAL positive_length_measure_with_unit;
section_modulii | : | ARRAY [1:8] OF modulus_measure_with_unit;
END_ENTITY;