This archive contains the CAD models for replicating the peg-in-hole test.

**Note: Diameter of CAD peg or hole may need to be adjusted based on the 3D printer in order to achieve a printed peg diameter of 14.8 mm and a printed hole diameter of 15.1 mm.