| 2012 Amendments |
| --- |
| The following table lists the codes, paragraphs, and pages in which the 97th National Conference on Weights and Measures made amendments. In the column headed “Action,” changes are noted as “added,” “amended,” “deleted,” or “renumbered.” Each code, section, or paragraph that has been changed will be noted as “Added 2012” or “Amended 2012.” |
| **SECTION** | **CODE** | **S&T****ITEM NO.** | **PARAGRAPH** | **ACTION** | **PAGE** |
| 2.20. | Scales | 320-3 | N.3.1. and N.3.1.1. | Amended Title | 2-31 |
| N.3.1.2. | Amended | 2-31 |
| 320-4 | Table T.1.1. | Amended | 2-36 |
| Table 7a. | Amended | 2-46 |
| UR.1.2. | Amended | 2-47 |
| 2.21. | Belt-conveyor Scale Systems | 321-1 | S.1.9. | Added | 2-60 |
| UR.3.1.(a)[[1]](#footnote-1) | Added | 2-69 |
| 321-2 | UR.1., UR.2., and UR.3. | Amended |  2-67 to 2-71 |
|  |  | UR.3.3. and UR.3.4. | Deleted |  2-69 to 2-71 |
| 3.30. | Liquid-Measuring Devices | 330-1 | S.1.6.4.1. | Amended | 3-08 |
| S.1.6.5.4. | Amended | 3-10 |
| S.1.6.6. | Amended | 3-11 |
| S.1.6.7. | Amended | 3-11 |
| S.1.6.8. | Added |  3-11 to  3-12 |
| UR.3.2. | Amended | 3-22 |
| UR.3.3. | Amended | 3-23 |
| 3.36. | Water Meters | 336-1 | S.3. and S.3.1. | Added | 3-97 |
| 5.58. | Multiple Dimension Measuring Devices | 358-1 | N.1.4.3. | Deleted | 5-79 |
| 5.59. | Electronic Livestock, Meat, and Poultry Evaluation Systems and/or Devices | 359-1 | Status of Code | “Tentative” status deleted from title.Preamble paragraph designating code as “Tentative” deleted. | 5-85 |
| Appendix D | Glossary | 320-6 | reference weight car | Amended | D-22 |

| 2012 Editorial Changes |
| --- |
| **SECTION** | **CODE** | **PARAGRAPH** | **ACTION** | **PAGE** |
| 1.10. | General | G-A.6. | Inserted the term “on or” following the word “enforceable” for consistency with nonretroactive dates throughout Handbook  44. | 1-3 |
| 2.20. | Scales | Table S.6.3.b., Note 13 | Following the term “e.g.,” reinserted the word “postal,” which was inadvertently deleted in the previous edition. | 2-24 |
| 2.21. | Belt-Conveyor Scale Systems | Table S.5. | Corrected Nonretroactive date to match the corresponding paragraph S.5. | 2-62 |
| 3.33. | Hydrocarbon Gas Vapor-Measuring Devices | S.1.1.3. (a) | Corrected metric equivalent of 10 000 ft3/h, which was incorrectly listed as 100 m3/h (rather than 280 m3/h) when SI units were added to NIST Handbook 44 in 1993. | 3-61 |
| S.1.1.3. | Delete the phrase “Volume-Measuring Devices.” This phrase was added in 1991 (along with a number of other changes) as part of S&T Item 333-1 to recognize mass flow meters. NCWM agreed to remove references to mass flow meters in individual codes in 1994 (S&T Item 337‑4A) when the Mass Flow Meters Code became a permanent code. | 3-61 |
| S.2.1. | Deleted phrase “Except when measured as a retail motor fuel” for the same reasons as described for S.1.1.3. above. | 3-63 |
| S.4.2. | Deleted the phrase “volume-measuring” for the same reasons as described for S.1.1.3. above. | 3-64 |
| UR.2.2. | Delete the phrase “for other than motor fuel” for the same reasons as described for S.1.1.3. above. | 3-66 |
| 3.34. | Cryogenic Liquid-Measuring Devices | Table N.4. | Updated publication references under “Hydrogen.” | 3-79 |

1. UR.3.1.(a) was numbered as UR.3.2.(a) under S&T Item number 321-1. Changes within the text caused the paragraphs to be renumbered. [↑](#footnote-ref-1)