time_measure_with_unit

EXPRESS specification:

ENTITY time_measure_with_unit
SUBTYPE OF ( | measure_with_unit);
WHERE
WRT4 | : | 'STRUCTURAL_FRAME_SCHEMA.TIME_UNIT' IN TYPEOF (SELF\measure_with_unit.unit_component);
WRT5 | : | 'STRUCTURAL_FRAME_SCHEMA.TIME_MEASURE' IN TYPEOF (SELF\measure_with_unit.value_component);
END_ENTITY;

References (6):

Name | Type | Referred through | Express-G
applied_load_dynamic | Entity |
Attribute 'load_duration'
| No Diagram
measure_with_unit | Entity |
Subtype
| No Diagram
project_plan_item | Entity |
Attribute 'item_duration'
| No Diagram
surface_treatment_thermal_timed | Entity |
Attribute 'time_to_maximum'
Attribute 'time_at_maximum'
Attribute 'time_to_final'
| No Diagram

Inheritance graph

ENTITY time_measure_with_unit;
ENTITY measure_with_unit;
value_component | : | measure_value;
unit_component | : | unit;
ENTITY time_measure_with_unit;
END_ENTITY;