surface_patch

EXPRESS specification:

ENTITY surface_patch;
parent_surface | : | bounded_surface;
u_transition | : | transition_code;
v_transition | : | transition_code;
u_sense | : | BOOLEAN;
v_sense | : | BOOLEAN;
INVERSE
using_surfaces | : | BAG [1:?] OF rectangular_composite_surface FOR segments;
WHERE
WRS35 | : | (NOT ('STRUCTURAL_FRAME_SCHEMA.CURVE_BOUNDED_SURFACE' IN TYPEOF(parent_surface)));
END_ENTITY;

References (2):

Name | Type | Referred through | Express-G
rectangular_composite_surface | Entity |
Attribute 'segments'
| No Diagram
select_generic_item | Select |
Select relation
| No Diagram

Inheritance graph

ENTITY surface_patch;
ENTITY surface_patch;
parent_surface | : | bounded_surface;
u_transition | : | transition_code;
v_transition | : | transition_code;
u_sense | : | BOOLEAN;
v_sense | : | BOOLEAN;
INVERSE
using_surfaces | : | BAG [1:?] OF rectangular_composite_surface FOR segments;
END_ENTITY;