element_surface

EXPRESS specification:

ENTITY element_surface
SUPERTYPE OF | (ONEOF(element_surface_simple, element_surface_complex))
SUBTYPE OF ( | element);
thickness | : | positive_length_measure_with_unit;
DERIVE
connectivities | : | SET [3:?] OF element_node_connectivity := bag_to_set (USEDIN(SELF,'STRUCTURAL_FRAME_SCHEMA.ELEMENT_NODE_CONNECTIVITY.CONNECTING_ELEMENT'));
WHERE
WRE14 | : | SELF\element.element_dimensionality = 2;
WRE15 | : | SELF\element.parent_model.coordinate_space_dimension > 1;
END_ENTITY;

References (4):

Name | Type | Referred through | Express-G
analysis_result_element_surface | Entity |
Attribute 'result_for_element_surface'
| No Diagram
element | Entity |
Subtype
| No Diagram
element_surface_complex | Entity |
Supertype
| No Diagram
element_surface_simple | Entity |
Supertype
| No Diagram

Inheritance graph

ENTITY element_surface;
ENTITY element;
element_name | : | label;
element_description | : | OPTIONAL text;
parent_model | : | analysis_model;
element_dimensionality | : | INTEGER;
INVERSE
connectivity | : | SET [1:?] OF element_node_connectivity FOR connecting_element;
ENTITY element_surface;
thickness | : | positive_length_measure_with_unit;
DERIVE
connectivities | : | SET [3:?] OF element_node_connectivity := bag_to_set (USEDIN(SELF,'STRUCTURAL_FRAME_SCHEMA.ELEMENT_NODE_CONNECTIVITY.CONNECTING_ELEMENT'));
END_ENTITY;