positive_length_measure_with_unit

EXPRESS specification:

ENTITY positive_length_measure_with_unit
SUBTYPE OF ( | measure_with_unit);
WHERE
WRP17 | : | 'STRUCTURAL_FRAME_SCHEMA.LENGTH_UNIT' IN TYPEOF (SELF\measure_with_unit.unit_component);
WRP18 | : | 'STRUCTURAL_FRAME_SCHEMA.POSITIVE_LENGTH_MEASURE' IN TYPEOF (SELF\measure_with_unit.value_component);
END_ENTITY;

References (132):

Name | Type | Referred through | Express-G
assembly_design_structural_member_linear_cambered_absolute | Entity |
Attribute 'absolute_offset_position'
| No Diagram
chemical_mechanism | Entity |
Attribute 'layer_thickness'
| No Diagram
element_surface | Entity |
Attribute 'thickness'
| No Diagram
fastener_simple | Entity |
Attribute 'nominal_diameter'
Attribute 'nominal_length'
| No Diagram
fastener_simple_bolt | Entity |
Attribute 'length_of_shank'
| No Diagram
fastener_simple_bolt_circular_head | Entity |
Attribute 'bolt_head_height'
Attribute 'head_diameter'
| No Diagram
fastener_simple_bolt_hexagonal_head | Entity |
Attribute 'bolt_head_height'
Attribute 'distance_across_vertices'
Attribute 'distance_across_flats'
| No Diagram
fastener_simple_bolt_square_head | Entity |
Attribute 'bolt_head_height'
Attribute 'distance_across_flats'
| No Diagram
fastener_simple_countersunk | Entity |
Attribute 'countersink_depth'
| No Diagram
fastener_simple_nut_circular | Entity |
Attribute 'outside_diameter'
| No Diagram
fastener_simple_nut_closed | Entity |
Attribute 'nut_depth'
| No Diagram
fastener_simple_nut_hexagonal | Entity |
Attribute 'distance_across_vertices'
Attribute 'distance_across_flats'
| No Diagram
fastener_simple_nut_square | Entity |
Attribute 'distance_across_flats'
| No Diagram
fastener_simple_screw | Entity |
Attribute 'screw_head_height'
| No Diagram
fastener_simple_screw_self_drilling | Entity |
Attribute 'pilot_hole_diameter'
Attribute 'drill_diameter'
| No Diagram
fastener_simple_screw_self_tapping | Entity |
Attribute 'pilot_hole_diameter'
| No Diagram
fastener_simple_stud | Entity |
Attribute 'thread_length_1'
Attribute 'thread_length_2'
Attribute 'length_of_shank'
| No Diagram
fastener_simple_washer | Entity |
Attribute 'inside_diameter'
Attribute 'external_dimension'
| No Diagram
fastener_simple_washer_load_indicating | Entity |
Attribute 'final_gap'
| No Diagram
feature_edge_chamfer_fillet | Entity |
Attribute 'edge_fillet_radius'
| No Diagram
feature_edge_chamfer_rounding | Entity |
Attribute 'edge_rounding_radius'
| No Diagram
feature_edge_chamfer_straight | Entity |
Attribute 'edge_chamfer_width'
Attribute 'edge_chamfer_depth'
| No Diagram
feature_thread | Entity |
Attribute 'thread_pitch'
Attribute 'thread_length'
| No Diagram
feature_volume_hole_circular | Entity |
Attribute 'hole_radius'
| No Diagram
feature_volume_hole_rectangular | Entity |
Attribute 'hole_length'
Attribute 'hole_height'
Attribute 'fillet_radius'
| No Diagram
feature_volume_hole_slotted | Entity |
Attribute 'slot_height'
Attribute 'slot_length'
| No Diagram
feature_volume_hole_slotted_curved | Entity |
Attribute 'curve_radius'
| No Diagram
feature_volume_prismatic_chamfer | Entity |
Attribute 'chamfer_length'
Attribute 'chamfer_depth'
| No Diagram
feature_volume_prismatic_flange_chamfer | Entity |
Attribute 'flange_chamfer_length'
Attribute 'flange_chamfer_width'
| No Diagram
feature_volume_prismatic_flange_notch | Entity |
Attribute 'flange_notch_length'
Attribute 'flange_notch_width'
Attribute 'flange_notch_radius'
| No Diagram
feature_volume_prismatic_notch | Entity |
Attribute 'notch_length'
Attribute 'notch_depth'
Attribute 'notch_radius'
| No Diagram
feature_volume_with_depth | Entity |
Attribute 'penetration_depth'
| No Diagram
grid_orthogonal | Entity |
Attribute 'spacing_1'
Attribute 'spacing_2'
| No Diagram
grid_skewed | Entity |
Attribute 'spacing_1'
Attribute 'spacing_2'
| No Diagram
measure_with_unit | Entity |
Subtype
| No Diagram
part_prismatic_simple | Entity |
Attribute 'cut_length'
Attribute 'stock_length'
Attribute 'x_offset'
| No Diagram
part_prismatic_simple_cambered_absolute | Entity |
Attribute 'absolute_offset_position'
| No Diagram
part_prismatic_simple_castellated | Entity |
Attribute 'end_post_width_1'
Attribute 'end_post_width_2'
Attribute 'castellation_spacing'
Attribute 'castellation_height'
Attribute 'castellation_width'
Attribute 'castellation_depth'
| No Diagram
part_sheet | Entity |
Attribute 'sheet_thickness'
| No Diagram
part_sheet_bounded_simple | Entity |
Attribute 'cut_y_dimension'
Attribute 'cut_z_dimension'
Attribute 'stock_y_dimension'
Attribute 'stock_z_dimension'
Attribute 'y_offset'
Attribute 'z_offset'
| No Diagram
section_profile_angle | Entity |
Attribute 'depth'
Attribute 'width'
Attribute 'thickness'
Attribute 'internal_fillet_radius'
Attribute 'edge_fillet_radius'
| No Diagram
section_profile_centreline | Entity |
Attribute 'thickness'
| No Diagram
section_profile_channel | Entity |
Attribute 'overall_depth'
Attribute 'flange_width'
Attribute 'flange_thickness'
Attribute 'web_thickness'
Attribute 'root_radius'
Attribute 'fillet_radius'
| No Diagram
section_profile_circle | Entity |
Attribute 'external_radius'
| No Diagram
section_profile_circle_hollow | Entity |
Attribute 'wall_thickness'
| No Diagram
section_profile_i_type | Entity |
Attribute 'overall_depth'
Attribute 'overall_width'
Attribute 'web_thickness'
Attribute 'flange_thickness'
Attribute 'internal_depth'
Attribute 'root_radius'
Attribute 'edge_radius'
| No Diagram
section_profile_i_type_asymmetric | Entity |
Attribute 'top_flange_width'
Attribute 'bottom_flange_width'
Attribute 'bottom_flange_thickness'
Attribute 'bottom_root_radius'
Attribute 'bottom_flange_edge_radius'
| No Diagram
section_profile_i_type_rail | Entity |
Attribute 'top_edge_radius'
Attribute 'bottom_edge_radius'
Attribute 'transition_radius_top'
Attribute 'transition_radius_bottom'
| No Diagram
section_profile_rectangle | Entity |
Attribute 'overall_depth'
Attribute 'overall_width'
Attribute 'external_fillet_radius'
| No Diagram
section_profile_rectangle_hollow | Entity |
Attribute 'wall_thickness'
Attribute 'internal_fillet_radius'
| No Diagram
section_profile_t_type | Entity |
Attribute 'overall_depth'
Attribute 'flange_width'
Attribute 'flange_thickness'
Attribute 'web_thickness'
Attribute 'root_radius'
Attribute 'edge_radius'
| No Diagram
section_properties | Entity |
Attribute 'surface_per_length'
Attribute 'radius_of_gyration_ry'
Attribute 'radius_of_gyration_rz'
| No Diagram
section_properties_asymmetric | Entity |
Attribute 'radius_of_gyration_ru'
Attribute 'radius_of_gyration_rv'
| No Diagram
surface_treatment_coat | Entity |
Attribute 'layer_thicknesses'
| No Diagram
weld_mechanism | Entity |
Attribute 'weld_dimension'
| No Diagram
weld_mechanism_fillet | Entity |
Attribute 'leg_length_y'
Attribute 'leg_length_z'
| No Diagram
weld_mechanism_fillet_intermittent | Entity |
Attribute 'fillet_weld_length'
Attribute 'fillet_weld_spacing'
| No Diagram
weld_mechanism_groove | Entity |
Attribute 'root_gap'
Attribute 'root_face'
| No Diagram
weld_mechanism_groove_beveled | Entity |
Attribute 'groove_depth'
Attribute 'groove_radius'
| No Diagram
zone_of_building_storey | Entity |
Attribute 'storey_height'
| No Diagram

Inheritance graph

ENTITY positive_length_measure_with_unit;
ENTITY measure_with_unit;
value_component | : | measure_value;
unit_component | : | unit;
ENTITY positive_length_measure_with_unit;
END_ENTITY;