applied_load_static_force

EXPRESS specification:

ENTITY applied_load_static_force
SUBTYPE OF ( | applied_load_static);
applied_force_fx | : | OPTIONAL force_measure_with_unit;
applied_force_fy | : | OPTIONAL force_measure_with_unit;
applied_force_fz | : | OPTIONAL force_measure_with_unit;
applied_moment_mx | : | OPTIONAL moment_measure_with_unit;
applied_moment_my | : | OPTIONAL moment_measure_with_unit;
applied_moment_mz | : | OPTIONAL moment_measure_with_unit;
WHERE
WRA14 | : | EXISTS (applied_force_fx) OR EXISTS (applied_force_fy) OR EXISTS (applied_force_fz) OR EXISTS (applied_moment_mx) OR EXISTS (applied_moment_my) OR EXISTS (applied_moment_mz);
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
applied_load_static | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY applied_load_static_force;
ENTITY applied_load;
applied_load_name | : | label;
ENTITY applied_load_static;
ENTITY applied_load_static_force;
applied_force_fx | : | OPTIONAL force_measure_with_unit;
applied_force_fy | : | OPTIONAL force_measure_with_unit;
applied_force_fz | : | OPTIONAL force_measure_with_unit;
applied_moment_mx | : | OPTIONAL moment_measure_with_unit;
applied_moment_my | : | OPTIONAL moment_measure_with_unit;
applied_moment_mz | : | OPTIONAL moment_measure_with_unit;
END_ENTITY;