section_profile_angle

EXPRESS specification:

ENTITY section_profile_angle
SUBTYPE OF ( | section_profile_simple);
depth | : | positive_length_measure_with_unit;
width | : | OPTIONAL positive_length_measure_with_unit;
thickness | : | positive_length_measure_with_unit;
internal_fillet_radius | : | OPTIONAL positive_length_measure_with_unit;
edge_fillet_radius | : | OPTIONAL positive_length_measure_with_unit;
leg_slope | : | OPTIONAL ratio_measure_with_unit;
DERIVE
width_value | : | REAL := NVL(width.value_component, depth.value_component);
WHERE
WRS5 | : | depth.value_component > thickness.value_component;
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
section_profile_simple | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY section_profile_angle;
ENTITY structural_frame_item;
item_number | : | INTEGER;
item_name | : | label;
item_description | : | OPTIONAL text;
DERIVE
item_ref | : | BAG OF identifier := get_item_ref(SELF);
cost_code | : | BAG OF label := get_item_cost_code(SELF);
object_id | : | globally_unique_id := get_instance_id(SELF);
ENTITY section_profile;
section_classification | : | OPTIONAL label;
cardinal_point | : | cardinal_point_ref;
mirrored | : | LOGICAL;
DERIVE
section_ref | : | BAG OF identifier := SELF\structural_frame_item.item_ref;
ENTITY section_profile_simple;
ENTITY section_profile_angle;
depth | : | positive_length_measure_with_unit;
width | : | OPTIONAL positive_length_measure_with_unit;
thickness | : | positive_length_measure_with_unit;
internal_fillet_radius | : | OPTIONAL positive_length_measure_with_unit;
edge_fillet_radius | : | OPTIONAL positive_length_measure_with_unit;
leg_slope | : | OPTIONAL ratio_measure_with_unit;
DERIVE
width_value | : | REAL := NVL(width.value_component, depth.value_component);
END_ENTITY;