applied_load_dynamic_acceleration

EXPRESS specification:

ENTITY applied_load_dynamic_acceleration
SUBTYPE OF ( | applied_load_dynamic);
preset_acceleration_ax | : | OPTIONAL linear_acceleration_measure_with_unit;
preset_acceleration_ay | : | OPTIONAL linear_acceleration_measure_with_unit;
preset_acceleration_az | : | OPTIONAL linear_acceleration_measure_with_unit;
preset_acceleration_arx | : | OPTIONAL rotational_acceleration_measure_with_unit;
preset_acceleration_ary | : | OPTIONAL rotational_acceleration_measure_with_unit;
preset_acceleration_arz | : | OPTIONAL rotational_acceleration_measure_with_unit;
WHERE
WRA11 | : | EXISTS (preset_acceleration_ax) OR EXISTS (preset_acceleration_ay) OR EXISTS (preset_acceleration_az) OR EXISTS (preset_acceleration_arx) OR EXISTS (preset_acceleration_ary) OR EXISTS (preset_acceleration_arz);
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
applied_load_dynamic | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY applied_load_dynamic_acceleration;
ENTITY applied_load;
applied_load_name | : | label;
ENTITY applied_load_dynamic;
initial_value | : | OPTIONAL applied_load_static;
final_value | : | OPTIONAL applied_load_static;
maximum_value | : | OPTIONAL applied_load_static;
minimum_value | : | OPTIONAL applied_load_static;
number_of_cycles | : | OPTIONAL count_measure;
load_duration | : | OPTIONAL time_measure_with_unit;
load_frequency | : | OPTIONAL frequency_measure_with_unit;
ENTITY applied_load_dynamic_acceleration;
preset_acceleration_ax | : | OPTIONAL linear_acceleration_measure_with_unit;
preset_acceleration_ay | : | OPTIONAL linear_acceleration_measure_with_unit;
preset_acceleration_az | : | OPTIONAL linear_acceleration_measure_with_unit;
preset_acceleration_arx | : | OPTIONAL rotational_acceleration_measure_with_unit;
preset_acceleration_ary | : | OPTIONAL rotational_acceleration_measure_with_unit;
preset_acceleration_arz | : | OPTIONAL rotational_acceleration_measure_with_unit;
END_ENTITY;