solid_replica

EXPRESS specification:

ENTITY solid_replica
SUBTYPE OF ( | solid_model);
parent_solid | : | solid_model;
transformation | : | cartesian_transformation_operator_3d;
WHERE
WRS27 | : | acyclic_solid_replica(SELF, parent_solid);
WRS44 | : | parent_solid\geometric_representation_item.dim = 3;
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
solid_model | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY solid_replica;
ENTITY representation_item;
name | : | label;
ENTITY geometric_representation_item;
DERIVE
dim | : | dimension_count := dimension_of(SELF);
ENTITY solid_model;
ENTITY solid_replica;
parent_solid | : | solid_model;
transformation | : | cartesian_transformation_operator_3d;
END_ENTITY;