part_prismatic_complex_tapered

EXPRESS specification:

ENTITY part_prismatic_complex_tapered
SUBTYPE OF ( | part_prismatic_complex);
taper_description | : | OPTIONAL text;
absolute_taper_1 | : | OPTIONAL length_measure_with_unit;
absolute_taper_2 | : | OPTIONAL length_measure_with_unit;
relative_taper_1 | : | OPTIONAL ratio_measure_with_unit;
relative_taper_2 | : | OPTIONAL ratio_measure_with_unit;
WHERE
WRP5 | : | EXISTS (absolute_taper_1) OR EXISTS (absolute_taper_2) OR EXISTS (relative_taper_1) OR EXISTS (relative_taper_2);
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
part_prismatic_complex | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY part_prismatic_complex_tapered;
ENTITY structural_frame_item;
item_number | : | INTEGER;
item_name | : | label;
item_description | : | OPTIONAL text;
DERIVE
item_ref | : | BAG OF identifier := get_item_ref(SELF);
cost_code | : | BAG OF label := get_item_cost_code(SELF);
object_id | : | globally_unique_id := get_instance_id(SELF);
ENTITY structural_frame_product;
life_cycle_stage | : | OPTIONAL label;
ENTITY part;
fabrication_method | : | fabrication_type;
manufacturers_ref | : | OPTIONAL text;
DERIVE
part_number | : | INTEGER := SELF\structural_frame_item.item_number;
part_name | : | label := SELF\structural_frame_item.item_name;
design_uses | : | SET OF design_part := bag_to_set (USEDIN(SELF,'STRUCTURAL_FRAME_SCHEMA.DESIGN_PART.DESIGN_PART_SPEC'));
physical_uses | : | SET OF located_part := bag_to_set (USEDIN(SELF,'STRUCTURAL_FRAME_SCHEMA.LOCATED_PART.DESCRIPTIVE_PART'));
ENTITY part_prismatic;
ENTITY part_prismatic_complex;
cross_sections | : | LIST [2:?] OF section_profile;
points_defining_part_axis | : | LIST [2:?] OF point_on_curve;
section_orientations | : | LIST [2:?] OF orientation_select;
DERIVE
number_of_sections | : | INTEGER := SIZEOF(cross_sections);
curve_defining_part | : | curve := points_defining_part_axis[1]\point_on_curve.basis_curve;
ENTITY part_prismatic_complex_tapered;
taper_description | : | OPTIONAL text;
absolute_taper_1 | : | OPTIONAL length_measure_with_unit;
absolute_taper_2 | : | OPTIONAL length_measure_with_unit;
relative_taper_1 | : | OPTIONAL ratio_measure_with_unit;
relative_taper_2 | : | OPTIONAL ratio_measure_with_unit;
END_ENTITY;