applied_load_static_pressure

EXPRESS specification:

ENTITY applied_load_static_pressure
SUBTYPE OF ( | applied_load_static);
applied_pressure_px | : | OPTIONAL pressure_measure_with_unit;
applied_pressure_py | : | OPTIONAL pressure_measure_with_unit;
applied_pressure_pz | : | OPTIONAL pressure_measure_with_unit;
WHERE
WRA15 | : | EXISTS (applied_pressure_px) OR EXISTS (applied_pressure_py) OR EXISTS (applied_pressure_pz);
END_ENTITY;

References (5):

Name | Type | Referred through | Express-G
applied_load_static | Entity |
Subtype
| No Diagram
load_element_distributed_surface_uniform | Entity |
Attribute 'load_value'
| No Diagram
load_element_distributed_surface_varying | Entity |
Attribute 'load_values'
| No Diagram
load_member_distributed_surface_uniform | Entity |
Attribute 'load_value'
| No Diagram
load_member_distributed_surface_varying | Entity |
Attribute 'load_values'
| No Diagram

Inheritance graph

ENTITY applied_load_static_pressure;
ENTITY applied_load;
applied_load_name | : | label;
ENTITY applied_load_static;
ENTITY applied_load_static_pressure;
applied_pressure_px | : | OPTIONAL pressure_measure_with_unit;
applied_pressure_py | : | OPTIONAL pressure_measure_with_unit;
applied_pressure_pz | : | OPTIONAL pressure_measure_with_unit;
END_ENTITY;