applied_load_dynamic

EXPRESS specification:

ENTITY applied_load_dynamic
SUPERTYPE OF | (ONEOF(applied_load_dynamic_acceleration, applied_load_dynamic_velocity))
SUBTYPE OF ( | applied_load);
initial_value | : | OPTIONAL applied_load_static;
final_value | : | OPTIONAL applied_load_static;
maximum_value | : | OPTIONAL applied_load_static;
minimum_value | : | OPTIONAL applied_load_static;
number_of_cycles | : | OPTIONAL count_measure;
load_duration | : | OPTIONAL time_measure_with_unit;
load_frequency | : | OPTIONAL frequency_measure_with_unit;
WHERE
WRA10 | : | EXISTS (initial_value) OR EXISTS (final_value) OR EXISTS (maximum_value) OR EXISTS (minimum_value) OR EXISTS (number_of_cycles) OR EXISTS (load_duration) OR EXISTS (load_frequency) OR ('STRUCTURAL_FRAME_SCHEMA.APPLIED_LOAD_DYNAMIC_ACCELERATION' IN TYPEOF (SELF)) OR ('STRUCTURAL_FRAME_SCHEMA.APPLIED_LOAD_DYNAMIC_VELOCITY' IN TYPEOF (SELF));
END_ENTITY;

References (3):

Name | Type | Referred through | Express-G
applied_load | Entity |
Subtype
| No Diagram
applied_load_dynamic_acceleration | Entity |
Supertype
| No Diagram
applied_load_dynamic_velocity | Entity |
Supertype
| No Diagram

Inheritance graph

ENTITY applied_load_dynamic;
ENTITY applied_load;
applied_load_name | : | label;
ENTITY applied_load_dynamic;
initial_value | : | OPTIONAL applied_load_static;
final_value | : | OPTIONAL applied_load_static;
maximum_value | : | OPTIONAL applied_load_static;
minimum_value | : | OPTIONAL applied_load_static;
number_of_cycles | : | OPTIONAL count_measure;
load_duration | : | OPTIONAL time_measure_with_unit;
load_frequency | : | OPTIONAL frequency_measure_with_unit;
END_ENTITY;