measure_with_unit

EXPRESS specification:

ENTITY measure_with_unit
SUPERTYPE OF | (ONEOF(length_measure_with_unit, mass_measure_with_unit, time_measure_with_unit, thermodynamic_temperature_measure_with_unit, plane_angle_measure_with_unit, solid_angle_measure_with_unit, area_measure_with_unit, volume_measure_with_unit, ratio_measure_with_unit, force_measure_with_unit, frequency_measure_with_unit, pressure_measure_with_unit, positive_length_measure_with_unit, derived_measure_with_unit, uncertainty_measure_with_unit));
value_component | : | measure_value;
unit_component | : | unit;
WHERE
WRM25 | : | valid_units (SELF);
END_ENTITY;

References (25):

Name | Type | Referred through | Express-G
area_measure_with_unit | Entity |
Supertype
| No Diagram
boundary_condition_spring_non_linear | Entity |
Attribute 'change_values'
| No Diagram
conversion_based_unit | Entity |
Attribute 'conversion_factor'
| No Diagram
currency_rate_with_unit | Entity |
Attribute 'per_quantity'
| No Diagram
derived_measure_with_unit | Entity |
Supertype
| No Diagram
force_measure_with_unit | Entity |
Supertype
| No Diagram
frequency_measure_with_unit | Entity |
Supertype
| No Diagram
length_measure_with_unit | Entity |
Supertype
| No Diagram
load_element_thermal | Entity |
Attribute 'temperature_gradients'
| No Diagram
mass_measure_with_unit | Entity |
Supertype
| No Diagram
measure_qualification | Entity |
Attribute 'qualified_measure'
| No Diagram
measure_select | Select |
Select relation
| No Diagram
physical_action | Entity |
Attribute 'basic_magnitude'
Attribute 'derived_magnitude'
| No Diagram
plane_angle_measure_with_unit | Entity |
Supertype
| No Diagram
positive_length_measure_with_unit | Entity |
Supertype
| No Diagram
pressure_measure_with_unit | Entity |
Supertype
| No Diagram
ratio_measure_with_unit | Entity |
Supertype
| No Diagram
release_spring_non_linear | Entity |
Attribute 'change_values'
| No Diagram
select_generic_item | Select |
Select relation
| No Diagram
solid_angle_measure_with_unit | Entity |
Supertype
| No Diagram
thermodynamic_temperature_measure_with_unit | Entity |
Supertype
| No Diagram
time_measure_with_unit | Entity |
Supertype
| No Diagram
uncertainty_measure_with_unit | Entity |
Supertype
| No Diagram
volume_measure_with_unit | Entity |
Supertype
| No Diagram

Inheritance graph

ENTITY measure_with_unit;
ENTITY measure_with_unit;
value_component | : | measure_value;
unit_component | : | unit;
END_ENTITY;