applied_load_dynamic_velocity

EXPRESS specification:

ENTITY applied_load_dynamic_velocity
SUBTYPE OF ( | applied_load_dynamic);
preset_velocity_vx | : | OPTIONAL linear_velocity_measure_with_unit;
preset_velocity_vy | : | OPTIONAL linear_velocity_measure_with_unit;
preset_velocity_vz | : | OPTIONAL linear_velocity_measure_with_unit;
preset_velocity_vrx | : | OPTIONAL rotational_velocity_measure_with_unit;
preset_velocity_vry | : | OPTIONAL rotational_velocity_measure_with_unit;
preset_velocity_vrz | : | OPTIONAL rotational_velocity_measure_with_unit;
WHERE
WRA12 | : | EXISTS (preset_velocity_vx) OR EXISTS (preset_velocity_vy) OR EXISTS (preset_velocity_vz) OR EXISTS (preset_velocity_vrx) OR EXISTS (preset_velocity_vry) OR EXISTS (preset_velocity_vrz);
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
applied_load_dynamic | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY applied_load_dynamic_velocity;
ENTITY applied_load;
applied_load_name | : | label;
ENTITY applied_load_dynamic;
initial_value | : | OPTIONAL applied_load_static;
final_value | : | OPTIONAL applied_load_static;
maximum_value | : | OPTIONAL applied_load_static;
minimum_value | : | OPTIONAL applied_load_static;
number_of_cycles | : | OPTIONAL count_measure;
load_duration | : | OPTIONAL time_measure_with_unit;
load_frequency | : | OPTIONAL frequency_measure_with_unit;
ENTITY applied_load_dynamic_velocity;
preset_velocity_vx | : | OPTIONAL linear_velocity_measure_with_unit;
preset_velocity_vy | : | OPTIONAL linear_velocity_measure_with_unit;
preset_velocity_vz | : | OPTIONAL linear_velocity_measure_with_unit;
preset_velocity_vrx | : | OPTIONAL rotational_velocity_measure_with_unit;
preset_velocity_vry | : | OPTIONAL rotational_velocity_measure_with_unit;
preset_velocity_vrz | : | OPTIONAL rotational_velocity_measure_with_unit;
END_ENTITY;