element_point_stationary_mass

EXPRESS specification:

ENTITY element_point_stationary_mass
SUBTYPE OF ( | element_point);
masses | : | ARRAY [1:3] OF REAL;
moments_of_inertia | : | ARRAY [1:3] OF ARRAY [1:3] OF REAL;
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
element_point | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY element_point_stationary_mass;
ENTITY element;
element_name | : | label;
element_description | : | OPTIONAL text;
parent_model | : | analysis_model;
element_dimensionality | : | INTEGER;
INVERSE
connectivity | : | SET [1:?] OF element_node_connectivity FOR connecting_element;
ENTITY element_point;
DERIVE
connectivities | : | BAG [1:1] OF element_node_connectivity := USEDIN(SELF,'STRUCTURAL_FRAME_SCHEMA.ELEMENT_NODE_CONNECTIVITY.CONNECTING_ELEMENT');
ENTITY element_point_stationary_mass;
masses | : | ARRAY [1:3] OF REAL;
moments_of_inertia | : | ARRAY [1:3] OF ARRAY [1:3] OF REAL;
END_ENTITY;