section_profile_i_type_asymmetric

EXPRESS specification:

ENTITY section_profile_i_type_asymmetric
SUBTYPE OF ( | section_profile_i_type);
top_flange_width | : | positive_length_measure_with_unit;
bottom_flange_width | : | positive_length_measure_with_unit;
bottom_flange_thickness | : | positive_length_measure_with_unit;
bottom_root_radius | : | OPTIONAL positive_length_measure_with_unit;
bottom_flange_slope | : | OPTIONAL ratio_measure_with_unit;
bottom_flange_edge_radius | : | OPTIONAL positive_length_measure_with_unit;
WHERE
WRS43 | : | (SELF\section_profile_i_type.overall_width :=: top_flange_width) OR (SELF\section_profile_i_type.overall_width :=: bottom_flange_width);
END_ENTITY;

References (2):

Name | Type | Referred through | Express-G
section_profile_i_type | Entity |
Subtype
| No Diagram
section_profile_i_type_rail | Entity |
Supertype
| No Diagram

Inheritance graph

ENTITY section_profile_i_type_asymmetric;
ENTITY structural_frame_item;
item_number | : | INTEGER;
item_name | : | label;
item_description | : | OPTIONAL text;
DERIVE
item_ref | : | BAG OF identifier := get_item_ref(SELF);
cost_code | : | BAG OF label := get_item_cost_code(SELF);
object_id | : | globally_unique_id := get_instance_id(SELF);
ENTITY section_profile;
section_classification | : | OPTIONAL label;
cardinal_point | : | cardinal_point_ref;
mirrored | : | LOGICAL;
DERIVE
section_ref | : | BAG OF identifier := SELF\structural_frame_item.item_ref;
ENTITY section_profile_simple;
ENTITY section_profile_i_type;
overall_depth | : | positive_length_measure_with_unit;
overall_width | : | positive_length_measure_with_unit;
web_thickness | : | positive_length_measure_with_unit;
flange_thickness | : | positive_length_measure_with_unit;
internal_depth | : | OPTIONAL positive_length_measure_with_unit;
flange_slope | : | OPTIONAL ratio_measure_with_unit;
root_radius | : | OPTIONAL positive_length_measure_with_unit;
edge_radius | : | OPTIONAL positive_length_measure_with_unit;
DERIVE
overall_depth_value | : | REAL := overall_depth.value_component;
overall_width_value | : | REAL := overall_width.value_component;
web_thickness_value | : | REAL := web_thickness.value_component;
flange_thickness_value | : | REAL := flange_thickness.value_component;
ENTITY section_profile_i_type_asymmetric;
top_flange_width | : | positive_length_measure_with_unit;
bottom_flange_width | : | positive_length_measure_with_unit;
bottom_flange_thickness | : | positive_length_measure_with_unit;
bottom_root_radius | : | OPTIONAL positive_length_measure_with_unit;
bottom_flange_slope | : | OPTIONAL ratio_measure_with_unit;
bottom_flange_edge_radius | : | OPTIONAL positive_length_measure_with_unit;
END_ENTITY;