pressure_measure_with_unit

EXPRESS specification:

ENTITY pressure_measure_with_unit
SUBTYPE OF ( | measure_with_unit);
WHERE
WRP19 | : | 'STRUCTURAL_FRAME_SCHEMA.PRESSURE_UNIT' IN TYPEOF (SELF\measure_with_unit.unit_component);
WRP20 | : | 'STRUCTURAL_FRAME_SCHEMA.PRESSURE_MEASURE' IN TYPEOF (SELF\measure_with_unit.value_component);
END_ENTITY;

References (18):

Name | Type | Referred through | Express-G
analysis_result_element_surface_stresses | Entity |
Attribute 'direct_stress_sigma_y'
Attribute 'membrane_stress_tau_yz'
Attribute 'direct_stress_sigma_z'
| No Diagram
analysis_result_element_volume_stress_tensor | Entity |
Attribute 'shear_stress_tau_zy'
Attribute 'shear_stress_tau_xz'
Attribute 'normal_stress_sigma_z'
Attribute 'normal_stress_sigma_y'
Attribute 'normal_stress_sigma_x'
Attribute 'shear_stress_tau_zx'
Attribute 'shear_stress_tau_yz'
Attribute 'shear_stress_tau_yx'
Attribute 'shear_stress_tau_xy'
| No Diagram
applied_load_static_pressure | Entity |
Attribute 'applied_pressure_px'
Attribute 'applied_pressure_py'
Attribute 'applied_pressure_pz'
| No Diagram
chemical_mechanism | Entity |
Attribute 'layer_design_strength'
| No Diagram
measure_with_unit | Entity |
Subtype
| No Diagram
weld_mechanism | Entity |
Attribute 'weld_design_strength'
| No Diagram

Inheritance graph

ENTITY pressure_measure_with_unit;
ENTITY measure_with_unit;
value_component | : | measure_value;
unit_component | : | unit;
ENTITY pressure_measure_with_unit;
END_ENTITY;