analysis_result_element_volume_stress_tensor

EXPRESS specification:

ENTITY analysis_result_element_volume_stress_tensor
SUBTYPE OF ( | analysis_result_element_volume);
shear_stress_tau_zy | : | pressure_measure_with_unit;
shear_stress_tau_xz | : | pressure_measure_with_unit;
normal_stress_sigma_z | : | pressure_measure_with_unit;
normal_stress_sigma_y | : | pressure_measure_with_unit;
normal_stress_sigma_x | : | pressure_measure_with_unit;
shear_stress_tau_zx | : | pressure_measure_with_unit;
shear_stress_tau_yz | : | pressure_measure_with_unit;
shear_stress_tau_yx | : | pressure_measure_with_unit;
shear_stress_tau_xy | : | pressure_measure_with_unit;
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
analysis_result_element_volume | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY analysis_result_element_volume_stress_tensor;
ENTITY analysis_result;
analysis_result_name | : | label;
sign_convention | : | OPTIONAL text;
results_for_analysis | : | analysis_method;
ENTITY analysis_result_element;
ENTITY analysis_result_element_volume;
result_for_element_volume | : | element_volume;
result_position | : | point;
position_label | : | OPTIONAL label;
ENTITY analysis_result_element_volume_stress_tensor;
shear_stress_tau_zy | : | pressure_measure_with_unit;
shear_stress_tau_xz | : | pressure_measure_with_unit;
normal_stress_sigma_z | : | pressure_measure_with_unit;
normal_stress_sigma_y | : | pressure_measure_with_unit;
normal_stress_sigma_x | : | pressure_measure_with_unit;
shear_stress_tau_zx | : | pressure_measure_with_unit;
shear_stress_tau_yz | : | pressure_measure_with_unit;
shear_stress_tau_yx | : | pressure_measure_with_unit;
shear_stress_tau_xy | : | pressure_measure_with_unit;
END_ENTITY;