feature_surface_with_layout

EXPRESS specification:

ENTITY feature_surface_with_layout
SUBTYPE OF ( | feature_surface);
layout | : | SET [2:?] OF point;
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
feature_surface | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY feature_surface_with_layout;
ENTITY structural_frame_item;
item_number | : | INTEGER;
item_name | : | label;
item_description | : | OPTIONAL text;
DERIVE
item_ref | : | BAG OF identifier := get_item_ref(SELF);
cost_code | : | BAG OF label := get_item_cost_code(SELF);
object_id | : | globally_unique_id := get_instance_id(SELF);
ENTITY feature;
DERIVE
uses | : | SET OF located_feature := bag_to_set (USEDIN(SELF,'STRUCTURAL_FRAME_SCHEMA.LOCATED_FEATURE.DESCRIPTIVE_FEATURE'));
ENTITY feature_surface;
ENTITY feature_surface_with_layout;
layout | : | SET [2:?] OF point;
END_ENTITY;