frequency_unit

EXPRESS specification:

ENTITY frequency_unit
SUBTYPE OF ( | named_unit);
WHERE
WRF27 | : | (SELF\named_unit.dimensions.length_exponent = 0.0) AND (SELF\named_unit.dimensions.mass_exponent = 0.0) AND (SELF\named_unit.dimensions.time_exponent = -1.0) AND (SELF\named_unit.dimensions.electric_current_exponent = 0.0) AND (SELF\named_unit.dimensions.thermodynamic_temperature_exponent = 0.0) AND (SELF\named_unit.dimensions.amount_of_substance_exponent = 0.0) AND (SELF\named_unit.dimensions.luminous_intensity_exponent = 0.0);
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
named_unit | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY frequency_unit;
ENTITY named_unit;
dimensions | : | dimensional_exponents;
ENTITY frequency_unit;
END_ENTITY;