material_anisotropic

EXPRESS specification:

ENTITY material_anisotropic
SUBTYPE OF ( | material);
properties | : | LIST [2:?] OF material_representation;
material_location | : | LIST [2:?] OF placement;
WHERE
WRM41 | : | SIZEOF(properties) = SIZEOF(material_location);
END_ENTITY;

References (1):

Name | Type | Referred through | Express-G
material | Entity |
Subtype
| No Diagram

Inheritance graph

ENTITY material_anisotropic;
ENTITY structural_frame_item;
item_number | : | INTEGER;
item_name | : | label;
item_description | : | OPTIONAL text;
DERIVE
item_ref | : | BAG OF identifier := get_item_ref(SELF);
cost_code | : | BAG OF label := get_item_cost_code(SELF);
object_id | : | globally_unique_id := get_instance_id(SELF);
ENTITY material;
DERIVE
material_number | : | INTEGER := SELF\structural_frame_item.item_number;
material_name | : | label := SELF\structural_frame_item.item_name;
material_grade | : | BAG OF identifier := SELF\structural_frame_item.item_ref;
ENTITY material_anisotropic;
properties | : | LIST [2:?] OF material_representation;
material_location | : | LIST [2:?] OF placement;
END_ENTITY;