inertia_measure_with_unit

EXPRESS specification:

ENTITY inertia_measure_with_unit
SUBTYPE OF ( | derived_measure_with_unit);
WHERE
WRI1 | : | 'STRUCTURAL_FRAME_SCHEMA.INERTIA_UNIT' IN TYPEOF (SELF\measure_with_unit.unit_component);
WRI2 | : | 'STRUCTURAL_FRAME_SCHEMA.INERTIA_MEASURE' IN TYPEOF (SELF\measure_with_unit.value_component);
END_ENTITY;

References (6):

Name | Type | Referred through | Express-G
derived_measure_with_unit | Entity |
Subtype
| No Diagram
section_properties | Entity |
Attribute 'torsional_constant_ix'
Attribute 'inertia_moment_iy'
Attribute 'inertia_moment_iz'
| No Diagram
section_properties_asymmetric | Entity |
Attribute 'inertia_moment_iu'
Attribute 'inertia_moment_iv'
| No Diagram

Inheritance graph

ENTITY inertia_measure_with_unit;
ENTITY measure_with_unit;
value_component | : | measure_value;
unit_component | : | unit;
ENTITY derived_measure_with_unit;
ENTITY inertia_measure_with_unit;
END_ENTITY;